|  |  |  |
| --- | --- | --- |
|  | | **Description** |
| Author(s)  Jokitulppo, Matti | Type of publication  Bachelor’s thesis | Date dd.mm.yyyy |
| Language of publication:  English |
| Number of pages  41 | Permission for web publication: x |
| Title of publication  **Arduino-controlled robot** | | |
| Degree programme  Software Engineering | | |
| Tutor(s)  Manninen, Pasi  Kotkansalo, Jouko | | |
| Assigned by  JAMK University of Applied Sciences | | |
| Abstract  The aim of this thesis was to create a Bluetooth controlled robot for JAMK University of Applied Sciences for marketing purposes. The robot is controlled via a Bluetooth LE link, from any Android phone or tablet using a custom application. The robot itself is controlled by an Arduino microcontroller, which in turn is controlled by the mobile application via a custom communications protocol.  This thesis contains a throughout description of the build process involved in the robot project, along with details and descriptions about the technological choices made on the assignment. Implementation of the project began first by researching possible technologies and sketching out the features the final product might have. After getting a clear picture of the desired end product, necessary components were ordered and assembled into a rough prototype. The Android mobile application and the embedded Arduino code were developed in tandem, implementing new features on both platforms as the time arose.  As a result of this thesis, the customer (JAMK) received a fully functional robot with companion app, which could easily be demonstrated in fairs or other similar events. It could be controlled using any Android compatible phone or tablet. | | |
| Keywords/tags ([subjects](http://www.nelliportaali.fi/V/?institute=JAMK&portal=JAMK&new_lng=eng&force_login=Y&func=find-db-1-category&mode=category&restricted=all&sequence=000013943))  Arduino, Bluetooth, Bluetooth LE, Android, Robot | | |
| Miscellaneous | | |

|  |  |  |
| --- | --- | --- |
|  | | **Kuvailulehti** |
| Tekijä(t)  Jokitulppo, Matti | Julkaisun laji  Opinnäytetyö | Päivämäärä pp.kk.vvvv |
| Sivumäärä  41 | Julkaisun kieli  Englanti |
|  | Verkkojulkaisulupa myönnetty: x |
| Työn nimi  **Arduino-controlled robot** | | |
| Koulutusohjelma  Ohjelmistotekniikan koulutusohjelma | | |
| Työn ohjaaja(t)  Manninen, Pasi  Kotkansalo, Jouko | | |
| Toimeksiantaja(t)  Jyväskylän ammattikorkeakoulu | | |
| Tiivistelmä  Tämän opinnäytetyön tavoitteena oli luoda yksinkertainen Bluetooth-kommunikaatiostandardin ylitse kontrolloitava robotti Jyväskylän Ammattikorkeakoululle markkinointitarkoituksiin. Robottia voidaan käskyttää millä tahansa Android-yhteensopivilla laitteella mobiilisovellusta hyödyntäen. Robottia itseään ohjaa Arduino-mikropiiri, jota sovellus käskyttää omalla protokollallaan muodostettuaan Bluetooth-linkin.  Tämä opinnäytetyö sisältää kattavan kuvauksen robottiprojektin rakennusprosessista, mukaanlukien kuvauksia projektin aikana tehdyistä teknologisista valinnoista. Toteutus aloitettiin aiemman prototyypin pohjalta tutkimalla uuteen robottiin tarvittavia ominaisuuksia ja komponentteja. Halutun lopputuloksen selkeennyttyä tarvittavat osat tilattiin ja koottiin valmiiksi lopputuotteeksi. Android-applikaatio ja robotin sulautettu sovellus tehtiin samanaikaisesti, toteuttaen uusia ominaisuuksia molemmilla alustoille tarpeen vaatiessa.  Tämän työn tuloksena tilaaja (Jyväskylän ammattikorkeakoulu) sai toimivan robotin ja mobiilisovelluksen, jonka avulla robottia voidaan helposti käskyttää ja esitellä messuilla tai muissa vastaavissa tilaisuuksissa. Sitä pystyy ohjaamaan millä tahansa Android-yhteensopivalla puhelimella tai tabletilla. | | |
| Avainsanat ([asiasanat](http://vesa.lib.helsinki.fi/))  Arduino, Bluetooth, Bluetooth LE, Android, Robotti | | |
| Muut tiedot | | |

Contents

[Glossary 4](#_Toc427411406)

[1 Introduction 7](#_Toc427411407)

[1.1 Project background and assignment 7](#_Toc427411408)

[1.2 The previous prototype 8](#_Toc427411409)

[1.2.1 Overview 8](#_Toc427411410)

[1.2.2 Features 9](#_Toc427411411)

[1.2.3 Components 9](#_Toc427411412)

[1.2.4 Android application 12](#_Toc427411413)

[1.3 Objectives for the new project 13](#_Toc427411414)

[2 Tools and technologies 14](#_Toc427411415)

[2.1 Arduino 14](#_Toc427411416)

[2.1.1 Introduction 14](#_Toc427411417)

[2.1.2 Arduino shields 15](#_Toc427411418)

[2.1.3 C++ and the Arduino language 15](#_Toc427411419)

[2.1.4 Arduino IDE 16](#_Toc427411420)

[2.2 Android 16](#_Toc427411421)

[2.2.1 Java 17](#_Toc427411422)

[2.2.2 Eclipse 17](#_Toc427411423)

[2.3 Version control and management 18](#_Toc427411424)

[2.3.1 Git 18](#_Toc427411425)

[2.3.2 GitHub 18](#_Toc427411426)

[3 The Android application 18](#_Toc427411427)

[3.1 Introduction 18](#_Toc427411428)

[3.2 Activities 19](#_Toc427411429)

[3.2.1 Settings activity 19](#_Toc427411430)

[3.2.2 Robot feed activity 21](#_Toc427411431)

[3.3 Application classes 23](#_Toc427411432)

[3.3.1 MjpegInputStream and MjpegView 23](#_Toc427411433)

[3.3.2 JoyStickView 24](#_Toc427411434)

[3.3.3 ApplicationState 24](#_Toc427411435)

[3.3.4 BluetoothStreamManager 24](#_Toc427411436)

[3.3.5 Feed 25](#_Toc427411437)

[3.3.6 Settings 25](#_Toc427411438)

[4 The robot 26](#_Toc427411439)

[4.1 Introduction 26](#_Toc427411440)

[4.2 Overview of robot parts 27](#_Toc427411441)

[4.2.1 Table of components 27](#_Toc427411442)

[4.2.2 Arduino Mega 2560 27](#_Toc427411443)

[4.2.3 Robot chassis 28](#_Toc427411444)

[4.2.4 Pan + tilt servo 28](#_Toc427411445)

[4.2.5 LiPo battery and UBEC 29](#_Toc427411446)

[4.2.6 Adafruit Motor Shield V2 29](#_Toc427411447)

[4.2.7 NeoPixel shield and matrix 30](#_Toc427411448)

[4.2.8 Emic 2 Text-to-speech module and speaker 30](#_Toc427411449)

[4.2.9 Raspberry Pi 2 with webcam 30](#_Toc427411450)

[4.3 Assembly 31](#_Toc427411451)

[5 The embedded program 32](#_Toc427411452)

[5.1 Introduction 33](#_Toc427411453)

[5.2 Communication between Android application and robot 34](#_Toc427411454)

[5.2.1 Motor command 34](#_Toc427411455)

[5.2.2 Message command 35](#_Toc427411456)

[6 Results and conclusion 36](#_Toc427411457)

[References 38](#_Toc427411458)

[Appendices 40](#_Toc427411459)

[Appendix 1. Robot parts diagram 40](#_Toc427411460)

**Figures**

Figure 1. Previous robot prototype 8

Figure 2. Pi-Lite LED shield on top of Raspberry Pi 11

Figure 3. Top-down view of old robot wiring 12

Figure 4. Old pin control activity 13

Figure 5. Arduino IDE 16

Figure 7. Settings activity 20

Figure 8. Robot feed activity 22

Figure 9. Robot message dialog 23

Figure 10. Finished robot 26

**Tables**

[Table 1. Robot parts and prices 27](#_Toc427411479)

# Glossary

**Arduino**

Arduino is a series of popular open-source microcontroller. Programmed using C or C++, it is intended to be an easy and inexpensive way for students and hobbyists to ease themselves into electronics. There exists a large variety of different add-ons and components to enhance the Arduino’s functionality.

**Bluetooth LE**

**Bluetooth Low Energy, also known as Bluetooth Smart, is a new, less power-intensive version of the existing Bluetooth standard, known today as Bluetooth Classic. Besides saving battery life, Bluetooth LE also promises less latency for most applications.**

**DC Motor**

A DC motor is a type of motor with a magnetic coil inside. When an electric current passes through the coil, the magnetic force generated proceeds to turn the motor. The current is passed through a commutator before entering the coil, which switches the direction of the current at the apex point, so the spinning continues. The speed of the motor can be controlled by limiting the current, and the direction is affected by the direction of the current.

**IDE**

An integrated development environment is a type of text-editor usually meant for source code. Besides editing text, IDEs often come bundled with a host of other features, such as a debugger, or a built-in compiler.

**LiPo Battery**

**Lithium polymer batteries are a type of batteries very popular in the world on remote controlled planes. They’re lightweight, hold a lot of capacity and are capable of discharging this capacity very quickly. (Understanding RC LiPo Batteries, 2015)**

**NeoPixel**

NeoPixel is a brand of individually addressable full-color RGB LEDs that can be controlled by a single input of a microcontroller.

**Raspberry Pi**

The Raspberry Pi is a small, cheap single-board computer. Originally meant as a teaching aid, it has gained much popularity in the hobbyist electronics community as being a portable, cheap solution to adding computing power to embedded projects. It runs its own modified distribution of the GNU/Linux operating system.

**RSSI**

**RSSI, short for ”Received Signal Strength Indicator” is the strength of a wireless connection, usually measured in dBm from 0 to -120db. The closer the value is to zero, the stronger the signal. (Speedguide.net)**

**Servo**

A servo is a special type of motor that is controlled by electronic pulses of varying lengths. The timing of these pulses tells the servo which position it should move to. Generating these pulses is extremely timing dependent, and therefore controlling them through normal computers is not recommended. Since operating systems with many processes taking up different amounts of resources at times, it is not guaranteed a length of code is always run at the same exact interval. This can cause the servo to jitter, since the timing may be off by a few tenths of a millisecond.

Most servos have a limited range of movement, usually from 0 to 180 degrees. There are many different kinds of servos on the market, from cheap and tiny ones to models costing up to hundreds of dollars, with features such as acceleration and temperature tracking and their own microcontrollers built in.

**SPI**

Serial Peripheral Interface is yet another serial data protocol popular with embedded systems. It consists of one master device (usually a microcontroller, such as an Arduino) that commands one or more other devices. (Arduino.cc, 2015)

**UART**

UART is a two-way serial communication protocol, which means there is no feasible way to communicate between more than two chips at the same time. It has two pins, TX (transmit) and RX (receive). Since there is no clock line, the data transfer amount per second must be negotiated in advance, before starting communications.

# Introduction

## Project background and assignment

In the winter of 2014 during an Android programming course held at JAMK University of Applied Sciences, an early prototype of the robot was built as the course’s mandatory final project. After the course it was suggested that a new version could be built specifically for JAMK. This new robot could be then used for marketing purposes in fairs, career days and such.

The new and improved robot would be built mostly with the same basic concepts as the earlier prototype. It would consist mostly of an Arduino microcontroller controlling a basic two-wheel hobbyist robot chassis. A small single-board computer called the Raspberry Pi would provide a live video feed via an on-board camera mounted on top of two servos, which can pan and tilt in almost every direction. The robot could be driven using an Android phone, tablet or other compatible device, over a Bluetooth connection. It could also transcribe speech utilizing a natural speech synthesis module.

After initial thesis-related meetings, it was decided that some of the more “technically oriented” features of the earlier robot could be cut on the whim of the builder. The main qualities the new prototype should focus on were agreed to be ease-of-use and visual impressiveness. To summarize, the goal of this thesis project is to build a functional, engaging remote-controlled robot for marketing purposes.

## The previous prototype

### Overview

The earlier robot, seen in figure 1, was mostly constructed out of excess components and materials left over from various other electronics projects. Exceptions to this are the two-wheel robot chassis itself, which lays the basis for all the other various parts, and the Adafruit Motor Shield, which is an add-on for the Arduino microcontroller used to better integrate various motors and servos into the robot. Those parts were purchased specifically for this project.



Figure 1. Previous robot prototype

### Features

When the old robot project was first starting out, the immediate end-goal was just to have a small vehicle of some sort that could be controlled through an Android application via Bluetooth. During the building process itself, many new ideas and functionalities were thought of and implemented, essentially on-the-fly. Soon after putting together the chassis and wiring up the wheels, it was noticed that the robot looked somewhat dull, and that it needed something extra to really make it memorable. In a previous project, the builder had used small LED matrixes to add animated eyes to a Halloween mask, and so it was decided that the robot could also use a pair of eyes for enhanced visual effect. Soon after the LED eyes came the idea of using another LED matrix for a mouth. This way, the robot could have a face of sorts.

After the robot got its face, it was decided that it would also need a voice. Since the LED matrix used for the mouth came with the functionality to scroll text on it, a way of sending messages from the Android application to this LED matrix through the Arduino was implemented. Afterwards, a small speaker was attached to the robot to provide audio effects while the text was being displayed.

As a somewhat late addition to the project a webcam streaming video to the application was added. This was simply because during testing it was found out that driving the robot was quite difficult if you could not see where you were going. A Raspberry Pi single-board computer was added to provide the functionality of recording video and sending it through WiFi.

### Components

The old robot and the new version share quite a lot of parts used in common. For example, both of them are built on top of the same two-wheeled robot chassis, which is then driven through the Adafruit Motor Shield. The two also have a similar approach to controlling the robot through the Android application, although the old model uses Bluetooth Classic, and the new version utilizes the somewhat newer Bluetooth LE standard of communication. Both of the robots also contain a Raspberry Pi streaming video footage through a webcam that is planted on top of the same make of servos. In fact, the webcam used in the new robot was the very same that was used in the old version, as it was originally borrowed from school and was seen to be a functional and proven solution.

The new robot utilizes the somewhat new NeoPixel brand of LEDs for its eyes and mouth. They sport features such as 255 different stages of brightness and a total RGB color space of 24 bits. Each NeoPixel “unit” come with their own separate LED driver, and they can be chained together to form complex light installations of varying shape and size. Meanwhile, the older robot uses two orange single-color 8x8 LED matrixes for the eyes, and a 14x9 red rectangular LED matrix called the Pi-Lite for the mouth, which can be seen in figure 2. As the name implies, the Pi-Lite is an add-on originally meant to be used together with a Raspberry Pi. However, it was repurposed for the old robot from a previous electronics project. The Pi-Lite interprets commands sent through simple UART, which means its usage is not strictly tied to any particular brand or type of microcontroller or computer. While the single-color LEDs of the old robot might not look as impressive or bright as the NeoPixels, they do have the advantage of using significantly less power.



Figure 2. Pi-Lite LED shield on top of Raspberry Pi

For communication the old robot uses the HC-05 serial Bluetooth module. The HC-05 is remarkably easy to use in embedded projects, as it does not require any additional libraries to function, and it sends data through UART, which means it only needs two pins, RX and TX to communicate data back and forth. Usability aside, the HC-05 can also be acquired for very cheap online, at least when compared to newer Bluetooth LE modules.

While the new robot contains a very sophisticated and expensive speech synthesis chip, the old robot had a comparatively simple piezo speaker to provide sound effects. Piezo speakers are very lightweight and small components made from a special ceramic material, which causes the speaker to vibrate when an electronic signal passes through it. This causes the speaker to emit sound waves, the frequency of which is affected by the frequency of the signal that passes through the piezo. Piezo speakers are used in many embedded applications, such as toys, for example. In the old robot, the speaker played a continuous robotic beeping tune when it was scrolling messages on the Pi-Lite.

The first robot was more of a proof-of-concept, and its development did not have any particular end goals or results in mind. New features were added at the whim of the builder. This had the unfortunate side-effect of the actual physical wiring of the robot becoming quite messy and unattractive in the end, as you can see in figure 3. More clean and organized schematics for the wiring were decided to be an important point to keep in mind when starting the new build.



Figure 3. Top-down view of old robot wiring

### Android application

As for the companion application used to control the robot itself, it was somewhat archaic in nature in its early versions. It used the default black-on-white styles of the Android environment, and contained many features that most people would find difficult to understand. Examples of such features are the ability to adjust the voltage of the Arduino’s pins, as you can see in figure 4. By itself, this feature does not achieve much, and it requires other elements such as LEDs to properly demonstrate its functionality. The simplicity of the end-user interface was due to the fact that the application would never be released to the public, and it only served a single purpose, to control the robot.



Figure 4. Old pin control activity

As was previously mentioned, the original robot was built as a final project for an Android programming course. Development of the Android application was started quite early during the course schedule, and the pitfalls and best practices in Android development were not yet fully known at the time. Thankfully, the Android side of the project was relatively small, and the lack of experience in mobile programming did not turn out to be too big of an issue.

## Objectives for the new project

During the initial thesis-related meetings, relatively large creative freedom was given with regards to the end product. However, it was decided that it would be very nice to have the mobile application also function properly on tablet devices. Furthermore, the two main requirements for the robot were agreed as ease-of-use and visual attractiveness. How these requirements should be fulfilled was not discussed at length.

It was decided that, as a technical experiment, the newly built robot would be built using Bluetooth Low Energy as the method of choice to transmit data between the mobile application and the microcontroller. The previous robot utilized the older Bluetooth Classic standard.

The main reason for this change was the promise of lower latency between the two systems, which would theoretically increase the responsiveness of the robot’s controls. The practical maximum speed packets could be transmitted with the previous prototype was once in around 115 milliseconds. Any faster output and the Arduino microcontroller could not keep up, and the packets would keep piling on in the serial buffer, which would eventually cause a fatal crash.

# Tools and technologies

## Arduino

### Introduction

Arduino is the name of an Italy-based popular electronics platform that aims to be as easy-to-use as possible. Both the hardware and software are completely open-source. It’s intended for easy and fast prototyping, and is mostly aimed towards aspiring students without a background in electronics or programming. (Arduino.cc, 2015).

Arduinos come in many different varieties. Most of them are based around the AVR-series of chips, which are manufactured by Atmel. While it’s these chips that provide all the real functionality, the Arduino board simply makes using them that much easier. It can be argued that, for experienced electronics users, the true value of Arduino comes not from the boards, but the entire open-source ecosystem that has grown around them, and all the libraries and communities they provide.

### Arduino shields

Arduino shields are pluggable add-ons that can be stacked on top of the Arduino board to further extend its capabilities (Arduino.cc, 2015). There exist hundreds of different kinds of shields on the market, both official and unofficial. They provide features such as wireless communication in the form of Wi-Fi or radio, easier communication with motors and servos, added sensors and much more.

### C++ and the Arduino language

C++ is an object-oriented superset of the C language, originally developed by Bjarne Stroustrup from 1979. (Learncpp.com, 2007). Since its inception, it has influenced many other programming languages, such as C# and Java. It is mostly designed for system programming and embedded, performance-intensive systems. (B. Stroustrup, 2014.)

While C++ is said to be a superset of the C language, The language used to program the Arduino family of microcontroller can be thought of as a subset of C++. While many of the familiar paradigms of C++ programming, such as object-oriented programming, are mostly too memory-intensive for embedded usage, is the Arduino language basically just a set of C/C++ functions.

The following is an example of a bare-minimum Arduino program:

The setup- and loop functions are the only two required functions that must always exist in a valid Arduino program. The setup function is called once, when the microcontroller is first powered up, at the beginning of the program. The program then proceeds to run forever inside the function called loop.

### Arduino IDE

The Arduino IDE is a multi-platform development platform for creating embedded programs that run on the many various Arduino microcontrollers. As you can see from Figure 4, it is rather basic in its functionality when compared to many other modern IDEs. However, for small-scale hobbyist projects its relative lack of modern features, such as code auto-completion, is not an issue.



Figure 5. Arduino IDE

## Android

Android is a very popular Linux-based operating system, specifically tailored for smartphones and tablets. It is estimated there are currently over one billion devices running Android in the world (Android.com, 2015).

Being based on Linux, Android is open-source technology. It is currently maintained by Google.

### Java

Much like C++, Java is also an object-oriented general purpose programming language (J. Gosling 2015). It was created by James Gosling in 1995, who was working for Sun Microsystems at the time. Sun Microsystems was acquired by Oracle Corporation in 2010, who have continued its development and maintenance ever since.

Java has quite a many uses, and one of the more popular uses is in programming mobile applications for the Android platform. In this particular project, the logic of the robot itself is programmed in C++ as mentioned before, and the mobile application used to control it is programmed in Java.

### Eclipse

Like the Arduino IDE, Eclipse is also a type of integrated development environment. While the Arduino IDE is mostly meant for beginners that are easing themselves into embedded programming, Eclipse attempts to target the enterprise audience. Eclipse is most known for its Java features, but it also supports many other languages, such as C++ or PHP in the form of plugins. (The Eclipse Foundation, 2015).

In this particular thesis project, Eclipse was used as the main platform for developing the Android application. However, it bears mentioning that since starting this project, Eclipse has been phased out by Google as the Android IDE of choice, in favor of their own IDE Android Studio (J. Eason, 2015). A switch to Android Studio wasn’t deemed necessary during this project, as the groundwork laid during the development of the previous robot was entirely made with Eclipse, and changing IDEs was deemed unnecessary.

## Version control and management

### Git

Git is a distributed, open-source version control system. Basically, Git works by saving and sending snapshots of a project to a remote repository. Other people can then commit and pull changes to this repository. Being distributed, with Git there is no urgent need for hosting a version management service online, because every Git repository contains the entire unabridged history of the project.

Git was originally created by Linus Torvalds, to aid in the development of the Linux kernel. Even though it is traditionally a command-line program, lacking a graphical interface, many such third-party programs have surfaced since Git’s inception.

### GitHub

GitHub is a social hosting service strictly for Git repositories. GitHub is a very popular medium for developers around the world to collaborate with each other on different projects. Users can create and host their own public Git repositories for free, but private repositories cost a monthly fee. Users can also interact with other users by contributing to their projects, for example, in the form of pull requests. Besides just hosting repositories, it also contains many additional features such as issue tracking, a wiki for documentation and enhanced pull request flow. (Github.com)

# The Android application

## Introduction

After much planning and testing, the final mobile application used to control the robot itself became quite simple in its functionality. A lot of features were dropped from the previous prototype (namely, the ability to control the voltage of the Arduino microcontroller’s different pins), because it was decided that they did not really fit the final purpose of the new robot prototype, namely being easy to use and looking pleasant. Also, a lot of the different configuration settings were dropped or heavily simplified, as they did not really bring any added value to the end-user.

The application itself consists of just two main activities. For all intents and purposes, in the context of Android programming one can think of activities to be the various different “screens” that make up a whole mobile application. When the user launches the application, they’re first greeted with a settings screen. After the user has paired their phone with the robot’s Bluetooth LE module, they can move on to the driving activity. Here they can control the robot with a joystick interface.

## Activities

### Settings activity

This is the view where the application starts in, so in essence you might call it the “main” activity of the whole application. As can be seen in figure 5, there are many different options you can configure through this particular activity. For example, the user can configure camera settings. Since the feed is sent via Wi-Fi, the IP address of the Raspberry Pi might not be the same in all cases. Therefore it makes the most sense to let the user configure the webcam IP address to whatever they wish. There is also the option to disable the video entirely, since during testing it was found out that it might slow down some older phones somewhat.



Figure 7. Settings activity

You can also change the update speed in milliseconds for the video feed view. This controls how often data is sent to the robot. Changing this to a lower number makes driving the robot feel more responsive, but setting it too low may cause the robot to act erratically if the Bluetooth module crashes due to too much data in its buffer. In the worst case scenario, this can lead to the robot driving out of control, and in need of being physically being restarted.

Below the video settings is a line of four buttons used to set up different emotes. Pressing these allow you to set up predetermined phrases for the robot to say, so on the robot feed activity you do not have to open up the message dialog every single time you want the robot to say something.

From the settings you can also pair with new Bluetooth devices. The dark gray button at the middle titled “Find devices” opens a pop-up window and initiates the discovery process for new Bluetooth devices and appends them to a list as they are found. From this list you can select devices and attempt to pair and form a connection, after which you can move on to the second activity.

After a successful connection to the robot has been formed, the user can move on to the next activity.

### Robot feed activity

This is the part of the application where most of the action happens. The majority of the activity is taken by the video feed, as can be seen in figure 6. There are some transparent controls located at the bottom. There are two “joysticks” on the bottom-left and bottom-right parts of the screen. The left joystick is used to control the movement of the robot. So for example, if the user pushes the left joystick to the left, the robot will start turning to the left. The right joystick is used to pan and tilt the camera around. The further away from the center of the joystick you pull the faster the robot will move.



Figure 8. Robot feed activity

The button on the bottom labeled “Message” opens up a simple dialog with a text box, as seen in figure 7. In it, you can type in text for the robot to display. This will cause the robot to actually speak the message out loud, using an on-board speech synthesis chip. The four other buttons labeled with “emote” can be used to make the robot say the predetermined phrases that were set in the settings screen.



Figure 9. Robot message dialog

There is also a simple indicator on the top left for the strength of the Bluetooth connection. Signal strength is received from the module as an RSSI (received signal strength indicator), which is then then calculated and shown to the user as a more intuitive percentage value.

## Application classes

### MjpegInputStream and MjpegView

The camera feed uses the popular MJPEG (Motion JPEG) format to read and handle data from the webcam server running on the Raspberry Pi. The Pi is hosting a GStreamer-pipeline, which is a popular open-source framework for handling multimedia of different kinds. MjpegInputStream is the bytestream that fetches data from the pipeline, and MjpegView is the UI widget which displays it. These two classes were taken from a GStreamer-specific fork of the original MJpegViewer-project for Android.

### JoyStickView

This is the joystick component, two of which are used on the video feed. They have an event-listener that updates on the joystick moving, and you can get their angle, power and direction out of it. This particular component is originally developed by GitHub-user Zerokol, with some modifications made here and there to ensure the best fit for the project at hand.

### ApplicationState

The primary functionality of the ApplicationState class is to pass a reference to the BluetoothStreamManager class around between different Activities. Generally speaking, in object-oriented programming languages such as Java, having a single large class such as this one is considered a bad practice. However, for such a small application such as this one, it was decided that this is an acceptable solution, since a complex object like the Bluetooth stream could not be passed between activities easily.

### BluetoothStreamManager

The main functionality of this class is ensuring data is properly transmitted to the robot. It offers a simple interface for common Bluetooth related actions such as connecting to a device, getting the strength and state of the Bluetooth connection, and transmitting data. The other activities of the application can then use this class to send commands to the Arduino, which are then captured in the device’s output.

The BluetoothStreamManager also holds a reference to the current activity, so it can display an error dialog if it loses connection to the Bluetooth module. This dialog prompts the user to return to Settings and attempt to repair devices.

In the previous iteration of the Android application, this class was quite a bit more complex. Activities using the class could not write data to the Arduino directly, but instead they would push data to a queue. A separate thread would then write the data from this queue to the output stream. This entire queue system was decided to be quite over-engineered for this particular use-case, since there was not really all that much data being transmitted between the different activities.

### Feed

This is the class corresponding to the Feed activity. Its main functionality is to send data to the Arduino every x milliseconds, where x is the update speed value specified on the settings screen. Data is transmitted as an array of bytes, with is then interpreted on the side of the embedded program. Most of the time, this byte array contains values that tell the robot what it should do in terms of movement. The two joysticks on the screen are used to get user input, which these motor valued are then calculated from. This communication protocol will be further extrapolated on in the upcoming sections.

The activity also contains a button that opens up a dialog where the user can send things for the robot to say. It also contains an implementation of the AsyncTask class, which is used to fetch the video feed asynchronously from the webcam, server, provided the user has previously enabled that particular feature in the settings activity.

### Settings

This class, corresponding to the Settings activity, simply keeps tabs on some different kinds of input fields used for configuration for the rest of the app. These settings are saved and loaded from Android’s SharedPreferences, which is a simple way to store values in between application sessions.

The other main functionality of this particular class worth mentioning is the pairing of Bluetooth devices, which is handled in this class. The user can press a button to initiate scanning for new, unknown devices. If any are found they’re then appended to the end of the list. Clicking on an item in the list initiates pairing with a Bluetooth device. The Bluetooth device is then paired with the phone and the output stream is passed on to BluetoothStreamManager, and the user can proceed to the stream activity.

# The robot

## Introduction

As one can see from figure 9, physically the new build of the robot looks quite similar to the old one. At a glance, the biggest physical differences are the new, larger eyes and mouth. Building the actual robot was a bit easier than in the previous project, as there was a much clearer general idea of parts needed and how they would fit together. Most of the new challenges in the actual building phase of the project came from the increased power requirements. All in all, building the new robot took about 50 hours, total.



Figure 10. Finished robot

## Overview of robot parts

### Table of components

Table 1 contains a short listing of all the different parts purchased during the project. Some of the parts were loaned from school for the purpose of this project, so their price is excluded from the listing. Refer to figure 9 to see how the parts come together to make the final build.

Table 1. Robot parts and prices

|  |  |
| --- | --- |
| **Part** | **Cost (€)** |
| Pan + tilt servo | 30 |
| 4000 mAh LiPo 7.2V battery + 5V/9A UBEC | 40,2 |
| 2 NeoPixel NeoMatrix 8x8 | 59 |
| NeoPixel Shield | 26,61 |
| Adafruit Motor Shield V2 | 17,56 |
| Emic 2 Text-to-Speech module | 59,95 |
| Small speaker | 1,95 |
| Robot chassis with motors | **56** |
| Bluetooth LE module (NRF8001) | 34,85 |
| Assorted wiring, resistors, etc. | 15 |
| Raspberry Pi 2 (Loaned from school) | N/A |
| Webcam (Loaned from school) | N/A |
| WiFi adapter | 20 |
| Arduino Mega | 45 |
|  | Total: 406,12 € |
|  |  |

### Arduino Mega 2560

Functioning as the “brains” of the robot is an Arduino Mega 2560 microcontroller. The Arduino handles essentially all the functionality, from animating the eyes and mouth and moving the wheels and servos to reading data from the Bluetooth module.

In the original project, the Arduino Uno was used. The Uno is slightly cheaper than the Mega, and comes with a bit less memory, pins and various other features. The small amount of memory in the Uno ended up being deciding factor for the upgrade, as it turns out the libraries needed to interface with the Bluetooth module and the NeoPixels needed a lot more memory than was anticipated. The Uno and the Mega both run at a clock rate of 16MHz, which means both are equally fast in terms of computing power.

### Robot chassis

This is the “body” of the robot, so to speak. The kit itself contains two cheap DC motors and a caster ball for movement, two metal plates with a variety of mounting holes and rails, a standard battery pack that can hold up to 5 AA batteries and a switch that is meant to be used to turn the aforementioned battery pack off and on.

This is the same hobby kit that was used in the previous prototype, as it had proved to be a good and affordable solution. However, the cheap motors ended up causing some issues, as when the robot reached a certain speed, they started to generate a critical amount of electrical noise which caused the Arduino to operate in an unstable manner. This was fixed quite easily by soldering some noise suppression capacitors to the motors and the metal chassis, to remove excess interference.

### Pan + tilt servo

Originally intended for mounting a security camera, this component consists of two servos laid on top of each other in a manner that allows a movement range of almost 360 degrees. Naturally, this range must be limited on the side of the embedded code, as otherwise the eye stalks could potentially get stuck on the wiring on the back of the robot.

On the top servo sits the webcam that is connected to the Raspberry. The two-servo system gives the camera a lot of flexibility, and allows it to capture video at a variety of different angles. The eyes and mouth are also mounted to the top servo.

### LiPo battery and UBEC

Nearly the whole robot is powered by a single 7.2 volt lithium polymer battery, originally designed for RC cars. The exceptions to this are the motors and the servos, which are powered from a different source. The reason for this is to avoid instability-causing voltage drops under heavy loads. While one is planning out a project that incorporates microcontrollers interacting with servos or motors or other “heavy-duty” components, one should always remember to separate their power supplies.

Since all the components are rated for 5 volts, the LiPo battery is connected to a Universal Battery Elimination Circuit. The purpose of this component is to take in a high amount of voltage, and then convert it to a steady output of 5 volts. This output can be then safely used without fear of burning out sensitive circuitry with too much voltage.

The components of the original robot were powered from a standard 5 volt USB power bank. This power bank was originally meant to be used to recharge mobile devices, but it served its role as a portable, easy-to-use power source quite adequately. The reason it was not used in the new robot was because its maximum output was only 3 amps, and the new robot uses quite a lot more than that at its peak consumption. The biggest reasons for this increased demand for power are the new RGB LEDs of the mouth and eyes. Each NeoPixel uses about 20 milliamps of current, and there are a total of 173 LEDs in this entire project. By itself, this totals up to a potential draw of 3.6 amperes.

### Adafruit Motor Shield V2

In this project an Arduino add-on called the Adafruit Motor Shield was used to control the various motors and servos. The main advantage of using a ready-made add-on such as the motor shield in is ease-of-use. Most of the “heavy lifting” can be safely left to the motor shield, and the builder doesn’t have to worry about issues such as protecting their microcontroller from unwanted power surges.

### NeoPixel shield and matrix

Purely for visual show, the robot contains a total of 173 full color LEDs. Two 8x8 matrixes form the robot’s eyes, and a 9x5 rectangular piece functions as its mouth. Mounted on top of two “stalks” cut from a plate of metal, the eyes blink and move around in a somewhat realistic fashion. The mouth also moves when the robot is talking.

### Emic 2 Text-to-speech module and speaker

The Emic 2 is a standalone voice synthesizer that takes in a stream of characters through UART, and then attempts to convert it to audible speech. This makes it quite easy to integrate into embedded projects, one need only to provide it with power and send serial data for it to pronounce. Naturally, the module also needs a small speaker attached to it to function as intended.

### Raspberry Pi 2 with webcam

The Raspberry Pi 2 is the newest model in the popular series of single-board computers made by the Raspberry Pi Foundation. For all intents and purposes, one can think of it as a small computer that has the ability to run custom distributions of the GNU/Linux operating system. The sole job of the Raspberry in this project is to host a GStreamer-based server that constantly outputs video from the on-board webcam. To aid in this task, the Raspberry also hosts its own Wi-Fi access point. If the user of the mobile application wants to access the video feed, they must first join this network the Pi is hosting.

In the original project, a Raspberry Pi 1 model B+ was used. The reason for this was simply that the new version was not available to the public at the time. Also in the original project the phone itself hosted the Wi-Fi access point, which the Raspberry would join. The reason for switching the hosting around is that it allows multiple devices to access the feed without restarting. It was also easy to forget to turn on your phone’s access point before starting the robot, which made the old system very unintuitive for the end-user.

Furthermore, one of the requirements for the new application was that it should be usable on tablets also. Since most Android tablet models cannot use SIM cards, they do not have access to the Internet through conventional means, and can only connect to a Wi-Fi access point, not host one. For most tablet users, this missing feature makes little to no difference, but not in this particular project.

## Assembly

In appendix 1, you can see the way that the finished robot is put together, and how all the interconnected parts communicate. This diagram is somewhat simplified when compared to the actual set-up, but it should give a concise overview of the robot. Probably the most blatant victim of oversimplification is the power management system. In reality, the UBEC does not just power the Arduino Mega, but also every single other component in the robot, from the Raspberry Pi to the Arduino. This visualization was intentionally left out from the diagram, simply because it would take too much space.

In practice, development of the robot was done in separate, isolated systems, which were tested and then finally integrated together into the finished version when they were functioning. For example, animating the various LEDs was developed entirely separately from the rest of the robot itself. During the development phase the Arduino Uno was used, as it was cheap and easy to acquire, and the large memory requirements of the final program did not come into play until it was time to finally put the whole program together.

Much like when building the earlier version, the project was begun by assembling the chassis. This task was quite easy, as it was the exact same platform that was used in the previous project. The same goes for the servos.

After the initial body of the robot was assembled, the next phase was to test out the Bluetooth LE module. Hooking it to the Arduino was not all that difficult. The bigger problems came on the Android side, when attempting to form a connection between the devices. Bluetooth LE is a relatively new technology, and its usage is more prevalent on Apple devices running the iOS operating system, so there were not a lot of examples on how to use it. It bears mentioning that, at this point in the project, the Arduino Uno was used, as the memory limitations were not realized during the early phases yet.

Working with the NeoPixels turned out to be quite easy, also. Much of the same animation code for the eyes could be reused from the previous robot. The mouth animations, however, had to be done from scratch, as the NeoPixel shield is just a LED regular matrix, and does not come with the same text-scrolling functionality as the previously used Pi-Lite. It was at this phase that the memory limitations of the Arduino Uno became apparent, and a switch to the more powerful Mega series was done.

After the LEDs were done, it was realized that the USB power bank with a maximum output of 3 amperes would simply not be powerful enough. Many alternative solutions for enhanced power output were looked into, such as adding another 5 AA battery pack. Ultimately the LiPo battery proved to be the optimal solution, as they are generally lightweight, cheap and can output a lot of current if needed. The only foreseeable downside to using LiPos is that they need a specialized charger, in order for them to be reused safely.

# The embedded program

## Introduction

In essence, the whole embedded program running on the Arduino is just a big state machine. The two main jobs of the embedded program are handling the animating of the eyes and mouth, and reading bytes from the Bluetooth module and reacting accordingly.

Like previously mentioned, all Arduino programs consist of a setup function which is run once, and a main loop which is run indefinitely after the setup. In this particular program, the setup function handles initializing the various components which together make up the robot. For example, it starts the serial connection to the text-to-speech chip and Bluetooth module, sets up the correct brightness and state for the various LEDs, and sets up the servos to their correct initial positions to make the robot face forwards.

The main loop checks for and reads bytes in the serial buffer of the Bluetooth module. It also handles the animations of the eyes and mouth, the latter only if the robot is currently “speaking” via the text-to-speech chip. The amount of time the mouth should be animated is calculated from the length of the message after it has been completely read from the Bluetooth module.

All in all, the robot has three possible states. These states are MOTOR, MESSAGE and NOTHING. With the exception of the “NOTHING”-state, these states directly correspond to the different kinds of messages the Android application can send. “NOTHING” just means that the program is currently idle, and is waiting for further input from the Android application.

If the robot is in “MOTOR”-state, it means that the next bytes it will receive will indicate the various speeds and states it should move its wheels and servos. Likewise, if the robot is in “MESSAGE”-state, it means that the all the incoming bytes should be interpreted as letters, which are then sent to the text-to-speech chip after a final delimiter has been received.

## Communication between Android application and robot

Every message send to the microcontroller is sent and read as arrays of bytes, as was outlined in the earlier chapter. For all intends and purposes, in the context of this application a byte can be thought of as a numeric value between 0 and 255. However, since bytes in the Java language are designed to be from -128 to 127, and the bytes in C++ are from 0 to 255, it was found out that they cannot be directly transmitted. To overcome this issue, the values sent from the Android application are from 0 to 127. They are multiplied by 2 on the Arduino side to get the correct values.

### Motor command

Here is an example of sending a simple movement command. The brackets represent the cells in the array, and the inner number represents their value:

[[123], [70], [64], [66], [127], [1]]

The first number is a simple delimiter, which lets the microcontroller know that the following five characters should be interpreted as a movement command, and not as anything else. Unlike for the other commands, there is no need for an ending delimiter, as the microcontroller itself knows that the robot command is only six bytes long.

The next byte tells the direction the leftmost motor should move in. This byte corresponds to either the ASCII character F for forward, B for backwards or R (82) for release, which is means the wheel should stay put. The third byte is the speed the leftmost motor should exert, from 0 to 127. In this example, the left motor is told to spin forward at half of its maximum speed.

The fourth and fifth numbers follow the same logic as the last two, except they’re for the right motor. In this case, the two numbers tell the motor to start moving backward at full speed.

The last character is related to positioning the two servos. It is a numbers from 0 to 9, which tells the two servos, which direction they should move to. This movement is relative to their current position. One can think of these as the eight cardinal directions, plus an extra value that means both servos should simply stay still.

### Message command

Compared to the motor command, sending messages for the text-to-speech module to pronounce is somewhat simpler. Since we are talking about text, the following example will present the bytes as their ASCII character equivalents.

z Hello! \n

The byte that corresponds to the letter z, which is 122, marks the start of a new displayable message. This delimiter is followed by an undefined amount of other characters, and finally the newline character to implicate that the message has ended, and is ready to be sent to the text-to-speech module via UART. Sending this particular series of bytes from the Android application would cause the robot to say the word “Hello” out loud.

As a limitation of sending each character as a regular byte, the robot’s means of communication is strictly restricted to ASCII characters. These characters are validated on the Android side before sending the message. The message is also limited to 40 characters, both on the Android and embedded side.

# Results and conclusion

When it comes to creative projects, it can sometimes be difficult to predict the quality and nature of the final outcome. The initial requirements, both functional and non-functional, were somewhat loose for this project. However, all things considered, the end result of this thesis far exceeded the expectations of the initial assignment.

Developing the application and embedded code itself was surprisingly easy. A lot of this had to do with the fact that much of the work in the planning stages could be adopted from the previous project.

The biggest difficulties were with utilizing Bluetooth LE on the Android side, as its support is relative new in the Android ecosystem, being supported only from Android 4.3 and upwards. This resulted in there not being a lot of documentation and examples and such. However, this was not a huge issue in the end. There were also some problems with setting up the Raspberry Pi 2 Wi-Fi access point, but this was resolved by switching the Wi-Fi adapter used to a different model.

Using Bluetooth LE for the communication between the application and the robot was an interesting experience. However, Bluetooth LE is mostly meant for devices that need to transmit data to the host device relatively rarely, which is not the case for this particular project, as it needs to transmit data every 200 milliseconds or so to maintain bearable latency from the perspective of the user. Also, as the name “Low Energy” implies, Bluetooth LE is intended for embedded devices with fairly restrictive power requirements such as heart trackers or other wearable technologies. The power consumption of the module is not really an issue in this case, since the difference between Bluetooth Classic and Bluetooth is still measured in dozens of milliamps, which do not really make a noticeable difference, compared to the LEDs for example. There is also the issue of cost and ease of implementation, as Bluetooth Classic modules can be acquired quite cheaply online, and there exists a wealth of documentation for their usage.

In the future, an interesting experiment would be to attempt an entirely Wi-Fi based communication method, an abandoning Bluetooth entirely. The Raspberry could run a web service that could be interacted with the Android application. The Pi would then be connected to the Arduino, and it could relay the bytes to the Arduino through UART. This could possibly increase the range of the robot by a few dozen meters or so. It is difficult to say how latency might be affected with a HTTP-based solution, but as an educated guess controlling the robot via Wi-Fi might cause some overhead, and therefore an increase in latency.

It would also be worthwhile to look into using other Bluetooth LE modules, mainly the nRF51822. They are sold by the brand name Bluefruit LE Friend by Adafruit, and they come in both SPI and UART variety. The nRF51822 is somewhat cheaper and a bit more powerful than the nRF8001. That aside, the more important distinction between the LE Friend and the currently used nRF8001-based module is the fact that the library used to interact with the LE Friend is significantly more compact. The Bluefruit library only takes about 426 bytes in total, while the nRF8001-based library is over twice as big, taking about 1,029 bytes. Changing modules would mean that the robot could switch back to using the Uno, as there would be no need for the extra memory of the Mega 2560. For reference, the Uno has a total amount of 2,048 bytes of dynamic memory, while the Mega 2560 has a maximum of 8,192 bytes.

All in all, both the customer and the builder consider this project and its end result to be a definite success. Hopefully it will inspire others to get into electronics and programming for many years to come.

# References

Understanding RC LiPo Batteries. Accessed on 27 July 2015. Retrieved from

http://www.rchelicopterfun.com/rc-lipo-batteries.html

Arduino.cc. What is Arduino? Accessed on 4 August 2015. Retrieved from https://www.arduino.cc/en/guide/introduction

Arduino.cc. A Brief Introduction to the Serial Peripheral Interface (SPI). Accessed on 5 August 2015. Retrieved from https://www.arduino.cc/en/Reference/SPI

Arduino.cc. Arduino Shields. Accessed on 4 August 2015. Retrieved from

https://www.arduino.cc/en/Main/arduinoShields

Android.com – History. Accessed on 4 August 2015. Retrieved from https://www.android.com/history/

The Eclipse Foundation. Desktop IDEs: Accessed on 4 August 2015. Retrieved from https://eclipse.org/ide/

Eason, J. 2015. The Android Developers Blog. Accessed on 4 August 2015. Retrieved from http://android-developers.blogspot.fi/2015/06/an-update-on-eclipse-android-developer.html

Stroustrup, B. 2014. Lecture: The essence of C++. Accessed on 29 July 2015. Retrieved from https://www.youtube.com/watch?v=86xWVb4XIyE

Learncpp.com, 2007. Introduction to C/C++. Accessed on 29 July 2015. Retrieved from http://www.learncpp.com/cpp-tutorial/03-introduction-to-cc/

Gosling, J.; Joy, B; Steele, G.; Bracha, G.; Buckley, A., 2015. The Java Language Specification. Accessed on 29 July 2015. Retrieved from https://docs.oracle.com/javase/specs/jls/se8/jls8.pdf

GitHub.com. Features. Accessed on 6 August 2015. Retrieved from https://github.com/features

Speedguide.net. How does RSSi (dBm) relate to signal quality (percent) ? Accessed on 8 August 2015. Retrieved from http://www.speedguide.net/faq/how-does-rssi-dbm-relate-to-signal-quality-percent-439

# Appendices

## Appendix 1. Robot parts diagram